;---------------------------------------------------------------------
;  Script file to create plots for dynamic problem
;    'Verification of FLAC-3D with SHAKE'
;     Linear Elastic Case, Model of Layered soil deposits
;---------------------------------------------------------------------

plot create plot Grid
plot add zone colorby group trans 80
plot set job on
plot create plot Acc_at_Base
plot add table ...
5               salias 'Base' linestyle color blue ...
                 xaxis Label 'Time (s)' ...
                 yaxis Label 'Acceleration (m/s/s)'
plot set outline false
plot set job on

plot create plot Acc_at_Midheight
plot add table ...
6               salias 'Midheight' linestyle color blue ...
               xaxis Label 'Time (s)' ...
               yaxis Label  'Acceleration (m/s/s)'
plot set outline false
plot set job on

plot create plot Acc_at_Ground_Surface
plot add table ...
7               salias 'Ground Surface' linestyle color blue ...
               xaxis Label 'Time (s)' ...
               yaxis Label  'Acceleration (m/s/s)'
plot set outline false
plot set job on

plot create plot Disp_at_Base
plot add table ...
8               salias 'Base' linestyle color blue ...
               xaxis Label 'Time (s)' ...
               yaxis Label  'Displacement (m)'
plot set outline false
plot set job on

plot create plot Rel_Disp_at_Midheight
plot add table ...
9               salias 'Midheight' linestyle color blue ...
               xaxis Label 'Time (s)' ...
               yaxis Label  'Relative Displacement (m)'
plot set outline false
plot set job on

plot create plot Rel_Disp_at_Ground_Surface
plot add table ...
10               salias 'Ground Surface' linestyle color blue ...
               xaxis Label 'Time (s)' ...
               yaxis Label  'Relative Displacement (m)'
plot set outline false
plot set job on

plot create plot StressStrain_at_Base
plot add table ...
2                salias 'Base' linestyle color blue  ...
               xaxis Label 'Shear strain (%)' ...
               yaxis Label 'Shear stress (kPa)'
plot set outline false
plot set job on

plot create plot StressStrain_at_Midheight
plot add table ...
3                salias 'Midheight' linestyle color blue  ...
               xaxis Label 'Shear strain (%)' ...
               yaxis Label 'Shear stress (kPa)'
plot set outline false
plot set job on

plot create plot StressStrain_at_Ground_Surface
plot add table ...
4                salias 'Ground Surface' linestyle color blue  ...
               xaxis Label 'Shear strain (%)' ...
               yaxis Label 'Shear stress (kPa)'
plot set outline false
plot set job on

plot create plot Conf_at_Base
plot add table ...
11               salias 'Base' linestyle color blue  ...
               xaxis Label 'Effective Confinement (kPa)' ...
               yaxis Label  'Shear Stress (kPa)'
plot set outline false
plot set job on

plot create plot Conf_at_Midheight
plot add table ...
12               salias 'Midheight' linestyle color blue  ...
               xaxis Label 'Effective Confinement (kPa)' ...
               yaxis Label  'Shear Stress (kPa)'
plot set outline false
plot set job on

plot create plot Conf_at_Ground_Surface
plot add table ...
13               salias 'Ground Surface' linestyle color blue  ...
               xaxis Label 'Effective Confinement (kPa)' ...
               yaxis Label  'Shear Stress (kPa)'
plot set outline false
plot set job on

plot create plot PP_at_Base
plot add table ...
14               salias 'Base' linestyle color blue  ...
               xaxis Label 'Time (s)' ...
               yaxis Label 'Pore Pressure (kPa)'
plot set outline false
plot set job on

plot create plot PP_at_Midheight
plot add table ...
15               salias 'Midheight' linestyle color blue  ...
               xaxis Label 'Time (s)' ...
               yaxis Label 'Pore Pressure (kPa)'
plot set outline false
plot set job on

plot create plot PP_at_Ground_Surface
plot add table ...
16               salias 'Ground Surface' linestyle color blue  ...
               xaxis Label 'Time (s)' ...
               yaxis Label 'Pore Pressure (kPa)'
plot set outline false
plot set job on

Return
